Table 3

Table 3. Comparison of the signal obtained with the surface coil and two solenoids exploring deep layers inside the core plug.

|  |  |  |
| --- | --- | --- |
| **Position of the spot (cm)** | **Probe** | **Echo signal (a.u.)** |
| 3 | sc | - |
| sol25 | 305 |
| 4.5 | sc | - |
| sol35 | 260 |